## com.gs.core.light

# GsLightsManager

apis for Gs keyboard light and notify led

### Supported Products:

All

# Detail

## Method

method | description
--- | ---
`public static` `GsLightsManager` `instance`(); |
`public` `void` `openCustom`(`int` color, `int` shineType); | open custom LED ### Params: color: should be one of COLOR_GREEN, COLOR_RED, COLOR_BLUE shineType: should be one of FLASHING_SPEED, FLASHING_SLOW, KEEPING_SHOW ### Supported Products: All
`public` `void` `closeCustom`(); | close custom LED ### Supported Products: All
`public` `void` `openKeyLed`(`int` keyLedType); | open key LED: mute, handset, handfree ### Supported Products: GXV3350
`public` `void` `closeKeyLed`(`int` keyLedType); | close key LED: mute, handset, handfree ### Supported Products: GXV3350

## Member & Constant

Member | description
--- | ---
`public static final` `int` `COLOR_GREEN` | ### Supported Products: All
`public static final` `int` `COLOR_RED` | ### Supported Products: All
`public static final` `int` `COLOR_BLUE` | ### Supported Products: All
`public static final` `int` `FLASHING_SPEED` | ### Supported Products: All
`public static final` `int` `FLASHING_SLOW` | ### Supported Products: All
`public static final` `int` `KEEPING_SHOW` | ### Supported Products: All
`public static final` `int` `KEY_TYPE_MUTE` | key LED type: mute ### Supported Products: GXV3350
`public static final` `int` `KEY_TYPE_HANDSET` | key LED type: handset ### Supported Products: GXV3350
`public static final` `int` `KEY_TYPE_HANDFREE` | key LED type: handfree ### Supported Products: GXV3350