## com.gs.scan.context

# ScanContext.ReceiveScanResult

Useful constants for receiving scan result. You can register a BroadcastReceiver with {@link #ACTION_SCANNER_RESULT} added intent-filter. And use the constants defined here to get the received scan information from the intent.

### Supported Products:

WP850

# Detail

## Method

method | description
--- | ---

## Member & Constant

Member | description
--- | ---
`public static final` `String` `SCAN_BARCODE1` | The first barcode. ### Supported Products: WP850
`public static final` `String` `SCAN_BARCODE2` | The second barcode. ### Supported Products: WP850
`public static final` `String` `SCAN_BARCODE_TYPE_NAME` | The name of the barcode type. ### Supported Products: WP850
`public static final` `String` `SCAN_STATE` | Scan result state. ### Supported Products: WP850
`public static final` `String` `SCAN_STATE_FAIL` | Scan state: Indicates scan failure. ### Supported Products: WP850
`public static final` `String` `SCAN_STATE_OK` | Scan state: Indicates successful scan. ### Supported Products: WP850